**20:10:36:40.  Tier 2 application completion.** The tier 2 interconnection process is complete when:

 (1)  All tier 2 screening criteria are satisfied and any minor EDS modifications are implemented;

 (2)  The small generator facility installation is approved by an electric code inspector with jurisdiction over the interconnection;

 (3)  The witness test, if conducted by the public utility, is successful;

 (4)  The parties execute a certificate of completion; and

 (5)  An interconnecting agreement has been executed.

 **Source:** 35 SDR 305, effective July 1, 2009.

 **General Authority:** SDCL 49-34A-27, 49-34A-93.

 **Law Implemented:** SDCL 49-34A-27, 49-34A-93.