**44:02:06:06.  Toilet and bathing facilities.** Soap, toilet tissue, and clean washcloths and towels must be provided for each guest or guest room. Hot and cold running water under pressure must be provided to each lavatory, shower, bathtub, and bathtub and shower combination. The hot water must be at a minimum of 110 degrees Fahrenheit and at a maximum temperature of 120 degrees Fahrenheit at the tap. Each shower, bathtub, and bathtub and shower combination shall be provided with individual control valves of the pressure balance, thermostatic, or combination pressure balance and thermostatic mixing valve type that provide scald and thermal shock protection. Bathing or shower facilities must have a nonslip floor surface such as a manufactured nonslip bathtub or shower unit, a rubberized throw mat, or adhesive-backed nonslip strips. All toilets, lavatories, and bathing fixtures must be kept clean, sanitary, and in good repair. Restroom fixtures must be cleaned and sanitized between guest stays.

**Source:** 23 SDR 75, effective November 19, 1996; 34 SDR 321, effective June 30, 2008.

**General Authority:** SDCL 34-1-17, 34-18-22.

**Law Implemented:** SDCL 34-18-22, 34-18-24.

**Cross-References:** State Plumbing Code, art 20:54.