**74:27:12:10.  Litter control devices.** MSWLFs must have litter control devices at the face of the unloading area and around the perimeter of the site. The litter control devices must be of sufficient size to control blowing litter.

**Source:** 17 SDR 8, effective July 26, 1990; 19 SDR 186, effective June 10, 1993.

**General Authority:** SDCL 34A-6-1.6.

**Law Implemented:** SDCL 34A-6-1.6.